Title: ECC/DEC/(05)05
Author: Josef Halamka
Last saved by: ORIS
Company: VÚS

Príloha č. 2

Zoznam relevantných predpisov a dokumentov

Por. č. | Označenie | Názov
1. | ECC/DEC/(05)05 | ECC Decision of 18 March 2005 on harmonised utilisation of spectrum for IMT-2000/UMTS systems operating within the band 2500-2690 MHz
2. | ECC/DEC/(05)01 | ECC Decision of 18 March 2005 on the use of the band 27.5-29.5 GHz by the Fixed Service and uncoordinated Earth stations of the Fixed-Satellite Service (Earth-to-space)
3. | ECC/DEC/(04)08 | ECC Decision of 9 July 2004 on the harmonised use of the 5 GHz frequency bands for the implementation of Wireless Access Systems including Radio Local Area Networks (WAS/RLANs)
4. | ECC/DEC/(04)06 | ECC Decision of 19 March 2004 on the availability of frequency bands for the introduction of Wide Band Digital Land Mobile PMR/PAMR in the 400 MHz and 800/900 MHz bands
5. | ECC/DEC/(02)06 | ECC Decision of 15 November 2002 on the designation of frequency band 2500-2690 MHz for UMTS/IMT-2000
6. | ERC/DEC(01)07 | ERC Decision of 12 March 2001 on harmonised frequencies, technical characteristics and exemption from individual licensing of Short Range Devices used for Radio Local Area Networks (RLANs) operating in the frequency band 2400 - 2483.5 MHz
7. | ERC/DEC(00)08 | ERC Decision of 19 October 2000 on the use of the band 10.7 - 12.5 GHz by the fixed service and Earth stations of the broadcasting-satellite and fixed-satellite Service (space-to-Earth)
8. | ERC/DEC(00)02 | ERC Decision of 27 March 2000 on the use of the band 37.5 - 40.5 GHz by the fixed service and Earth stations of the fixed - satellite service (space to Earth)
9. | ERC/DEC(99)15 | ERC Decision of 1 June 1999 on the designation of the harmonised frequency band 40.5 to 43.5 GHz for the introduction of Multimedia Wireless Systems (MWS) including Multipoint Video Distribution Systems (MVDS)
10. | ERC/DEC(99)25 | ERC Decision of 29 November 1999 on the harmonised utilisation of spectrum for terrestrial Universal Mobile Telecommunications System (UMTS) operating within the bands 1900 - 1980 MHz, 2010 - 2025 MHz and 2110 - 2170 MHz
11. | ERC/DEC(97)02 | ERC Decision of 21 March 1997 on the extended frequency bands to be used for the GSM Digital Pan-European Communication System
12. | ERC/DEC(97)07 | ERC Decision of 30 June 1997 on the frequency bands for the introduction of the Universal Mobile Telecommunications System (UMTS)
13. | ERC/DEC(95)03 | ERC Decision of 1 December 1995 on the frequency bands to be designated for the introduction of DCS 1800
14. | ERC/DEC(94)01 | ERC Decision of 24 October 1994 on the frequency bands to be designated for the coordinated introduction of the GSM digital pan-European communications system
15. | ECC/REC 04-06 | Guidelines for block allocation for Fixed Wireless systems in the band 31.8-33.4 GHz
16. | ECC/REC 02-02 | Channel arrangements for digital fixed service systems (point-to-point and point-to-multipoint) operating in the frequency band 31 – 31.3 GHz
17. | ERC/REC 01-02 | Preferred channel arrangement for digital fixed service systems operating in the frequency band 31.8 - 33.4 GHz
18. | ERC/REC 00-05 | Use of the band 24.5 - 26.5 GHz for fixed wireless access
19. | ERC/REC 01-03 | Use of parts of the band 27.5-29.5 GHz for Fixed Wireless Access (FWA)
20. | ERC/REC 01-04 | Recommended guidelines for the accommodation and assignment of Multimedia Wireless Systems (MWS) in the frequency band 40.5 – 43.5 GHz
21. | ERC/REC 14-01 | Radio-frequency channel arrangements for high capacity analogue and digital radio-relay systems operating in the band 5925 MHz - 6425 MHz
22. | ERC/REC 14-02 | Radio-frequency channel arrangements for medium and high capacity analogue or high capacity digital radio-relay systems operating in the band 6425 MHz - 7125 MHz
23. | ERC/REC 13-04 | Preferred frequency bands for fixed wireless access in the frequency range between 3 and 29.5 GHz
24. | ERC/REC 12-08 | Harmonised radio frequency channel arrangements and block allocations for low, medium and high capacity systems in the band 3600 MHz to 4200 MHz

25.

ERC/REC 70-03

Relating to the use of Short Range Devices (SRD) 
Implementation status see the attached file REC7003IMPL.PDF 
No information in implementation use download

26. | T/R 13-02 | Preferred channel arrangements for fixed services in the range 22.0-29.5 GHz
27. | ECC REPORT 25 | The European table of frequency allocations and utilisations covering the frequency range 9 kHz to 275 GHz
28. | ECC REPORT 068 | Compatibility studies in the band 5725-5875 MHz between Fixed Wireless Access (FWA) systems and other systems
29. | CCIR REC 385-6 | Frekvenčný plán pre rádioreléové spoje bod – bod v pásme horné 7 GHz
30. | 2002/20/EC | Directive 2002/20/EC of the European Parliament and of the Council, of 7 March 2002 - on the authorisation of electronic communications networks and services (Authorisation Directive)
31. | 2002/21/EC | Directive 2002/21/EC of the European Parliament and of the Council, of 7 March 2002 - on a common regulatory framework for electronic communications networks and services (Framework Directive)
32. | 2002/622/EC | Decision no. 676/2002/EC of the European Parliament and of the Council, of 7 March 2002 - on a regulatory framework for radio spectrum policy in the European Community (Radio Spectrum Decision)
33. | 676/2002/EC | Decision no. 676/2002/EC of the European Parliament and of the Council, of 7 March 2002 - on a regulatory framework for radio spectrum policy in the European Community (Radio Spectrum Decision)
34. | 1999/EC/EC | Directive 1999/5/EC of the European Parliament and of the Council, of 9 March 1999 on radio equipment and telecommunications terminal equipment and the mutual recognition of their conformity
35. | 87/372/EEC | Council Directive of 25 June 1987 on the frequency bands to be received for the coordinated introduction of public pan-European cellular digital land-based mobile communications in the Community
36. | COM (2005) 204 final | Communication from the Commission to the Council, the European Parliament, the European Economic and Social Committee and the Committee of the Regions on accelerating the transition from analogue to digital broadcasting

37.

Dohoda
(Berlín 2003)

Agreement between the Administrations of…. on the co-ordination of frequencies between 29.7 MHz and 39.5 GHz for the fixed service and the land mobile service. Berlin, 28 November 2003

38. | ST 61 | The "Regional Agreement for the European Broadcasting Area Concerning the Use of Frequencies by the Broadcasting Service in the VHF and UHF Bands" adopted by the European VHF/UHF Broadcasting Conference (Stockholm, 1961)
39. | Ch 97 | Mnohostranná koordinačná dohoda (Chester 1997) o technických kritériách, zásadách koordinácie a postupoch pri zavádzaní pozemského digitálneho televízneho vysielania (DVB-T). Chester, 25. júla 1997
40. | Nariadenie vlády SR č. 443/2001 Z. z. | Nariadenie vlády 443/2001 Z. z., ktorým sa ustanovujú podrobnosti o technických požiadavkách a postupoch posudzovania zhody na rádiové zariadenia a koncové telekomunikačné zariadenia
41. | Uznesenie vlády SR č. 589 | Uznesenie vlády Slovenskej republiky č. 589 z 27. júna 2001 k stratégii a technickým kritériám na zavedenie pozemského digitálneho TV vysielania v systéme DVB-T na Slovensku
42. | Zákon NR SR č. 610/2003 Z. z. | Zákon č. 610/2003 Z. z. o elektronických komunikáciách v znení neskorších predpisov
43. | Zákon NR SR č. 308/2000 Z. z. | Zákon č. 308/2000 Z. z. o vysielaní a retransmisii v znení neskorších predpisov